This program loads a file named "CONFIG.CSV" when started.  This file contains the most recent configuration data for this site.  If this file isn't found or has been corrupted, simply re-enter your serial port and site settings and resave the configuration.  A new CONFIG.CSV file will be created!
To connect to a site, select Connect from the main pull down menu.  The last configured site will be displayed, ready to connect.
This program also supports direct connection to a peaker switch or soft-load transfer switch.  Use this connection with a Ethernet terminal server.  This permits a direct connection via a LAN, eliminating the need for a dial-up modem connection.
You can contact Cutler-Hammer for assistance with this program at  +1 724 773 1216.
The VB source code for this program is included on the installation disk, but is not installed by default.
This program, by default, monitors the modem for any incoming calls from a remote alarm dialer.  To disable this function, select View from the main pull down menu, then uncheck the "enable" checkbox next to the choice "Listen for incoming alarms".
The system defaults to "Standard" logging.  In this mode, the various setup strings sent to the modems are not displayed in the log files.  If you are having troubles with the modem either dialing or answering calls, select "Detailed" logging from the File / Properties / Port pull down menu.
When the optional alarm dialer is included at the site, that dialer will send a message to this program, then hold the line open for 60 seconds waiting for another alarm message (that way it won't have to redial).  However, if no additional alarms arrive, the incoming line appears to go dead.  No problem.  Just wait for 60 seconds (see the hang up message on the status screen to be sure).
If you attempt to dial out to a site while the site is receiving an alarm message, the connect will fail.  If you wish to terminate the incoming alarm (not recommended), you may do so by pressing the "Disconnect" button under the CONNECT option of the pull down menu.  At this point, you can then dial out to a remote site.
When exiting from the Site Status window (accessed from the Connect pull-down menu on the main screen), the system will automatically re-enable the "Monitor" check box of the Configure Port properties.  This means that even if you have disabled monitoring of incoming alarms, it will be activated by default once you disconnect from a site.
